**EXPOLIGHT**

**Projector equipped with a 50 cm rod and an adjustable 270° anti-glare head,  
Tiltable up to 90 °.  
The fixture’s head integrates an LED COB as well as a high efficiency reflector.**

**Passive thermal dissipation through external heatsink, thus ensuring the longevity of the LED.  
Light fitting equipped with a clamping fixing system with tightening screw, for panels from 20 to 45mm.**

**LED Driver Box equipped with 2 JST18 input/output WIELAND connectors for chained power supplies (up to 30 spotlights).  
Supplied without 230V power cable (see accessories).**

**Option: Dimming potentiometer (larger box). Available in Duo version for 2-sided panels.**