**MOOVEO HR**

**Track or surface mounted mini spotlight, high performance, high Led output, focusable and on-board dimming.  
Track mounted (1 circuit – 12V), surface mounted or Jack fitted.**

**Inclinaison +/- 135°. Rotation : 350°.**